


Step 1:open My Computer - Management - Device Manager - Universal Serial Bus Controller-USB Device-Browse Import Drivers(PhoenixSuitV1.10)





Step 2:Find out and decompress the PhoenixSuitV1.10.rar, install PhoenixSuit







Step 3:Open the PhoenixSuit:



Step 4:Click the icon and switch to firmware panel,then click import the firmware







Step 4: (1)Prepare a cable with 2 USB connectors.

first of all，USB connector to connect your computer.

(2)Use toothpick or needle to stick in the AV interface,Press the Reset button,Don’t let go. Then ,please hold on pressing it Use 1 USB connector to connect the USB2(attention!) on the Android TV box.



Step 5:please click YES(是），then the PhoneixSuit will work.,and you can release the reset button.When it shows 100% :Burning successfully, it means the Burning Procedure finished successfully.



